

Renewable Energy (Electricity) Amendment Regulation (No. 5)1

Select Legislative Instrument 2012 No. 127

I, QUENTIN BRYCE, Governor-General of the Commonwealth of Australia, acting with the advice of the Federal Executive Council, make the following regulation under the *Renewable Energy (Electricity) Act 2000*.

Dated 28 June

QUENTIN BRYCE

Governor-General

By Her Excellency’s Command

GREG COMBET

Minister for Climate Change and Energy Efficiency

1 Name of regulation

This regulation is the *Renewable Energy (Electricity) Amendment Regulation 2012 (No. 5)*.

2 Commencement

This regulation commences on the day after it is registered.

3 Amendment of *Renewable Energy (Electricity) Regulations 2001*

Schedule 1 amends the *Renewable Energy (Electricity) Regulations 2001*.

Schedule 1 Amendments

(section 3)

[] Paragraph 22X (1B) (b)

omit

43

insert

44

[] Schedule 6, after Part 43

insert

Part 44 Manufacture of reconstituted wood‑based panels

Division 1 Manufacture of reconstituted wood‑based panels

728 Manufacture of reconstituted wood‑based panels

The manufacture of reconstituted wood‑based panels is the physical and chemical transformation of wood, including wood particles and residues (such as chips, shavings and sawdust) into a reconstituted wood-based panel that:

(a) has a density of greater than 500 kg a cubic metre; and

(b) has individual wood particles or fibres with an average maximum dimension of no more than 30 mm.

Examples of reconstituted wood-based panels are particleboard and medium density fibreboard.

Division 2 Classification of activity

729 Classification of activity

The manufacture of reconstituted wood‑based panels is a moderately emissions‑intensive activity.

Division 3 Electricity baseline for calculating partial exemption

730 Electricity baseline for product

The electricity baseline for calculating the amount of a liable entity’s partial exemption in respect of the manufacture of reconstituted wood‑based panels is 0.372 MWh per tonne of raw reconstituted wood-based panel that:

(a) has a density of greater than 500 kg a cubic metre; and

(b) has individual wood particles or fibres with an average maximum dimension of no more than 30 mm; and

(c) is produced by carrying on the emissions-intensive trade-exposed activity; and

(d) is of saleable quality.

*Note*  ***Saleable quality*** is defined in regulation 22C.

**Note**

1. All legislative instruments and compilations are registered on the Federal Register of Legislative Instruments kept under the *Legislative Instruments Act 2003.* See [www.comlaw.gov.au](http://www.comlaw.gov.au/).