

Vehicle Standard (Australian Design Rule 42/04 – General Safety Requirements) 2005 Amendment 6

I, PAUL FLETCHER, Minister for Territories, Local Government and Major Projects, determine this vehicle standard under section 7 of the *Motor Vehicle Standards Act 1989*.

Dated 2 February 2016

[SIGNED]

Paul Fletcher

Minister for Territories, Local Government and Major Projects

**CONTENTS**

[1. Legislative provisions 3](#_Toc256000003)

[2. Amendment of vehicle standard 3](#_Toc256000004)

[Schedule 1 3](#_Toc256000005)

## Legislative provisions

* 1. Name of Legislative Instrument
     1. This instrument is the Vehicle Standard Australian Design Rule 42/04 –General Safety Requirements 2005 Amendment 6
  2. Commencement
     1. This instrument commences on the day after it is registered.

## Amendment of vehicle standard

* 1. The changes specified in Schedule 1 amend Vehicle Standard (Australian Design Rule 42/04 – General Safety Requirements) 2005.

## Schedule 1

1. Clause 8.1.2 amended to read:

“the bumper contact surface is located not more than 600 mm forward of the rear of the vehicle;”