

Radiocommunications (Citizen Band Radio Stations) Class Licence Variation 2017 (No. 1)

The Australian Communications and Media Authority makes the following Variation under subsection 132(1) of the *Radiocommunications Act 1992*.

Dated: 6 April 2017

Richard Bean

[signed]

Member

James Cameron

[signed]

Member/~~General Manager~~

Australian Communications and Media Authority

1 Name

 This is the *Radiocommunications (Citizen Band Radio Stations) Class Licence Variation 2017 (No. 1)*.

2 Commencement

 This Variation commences at the start of the day after it is registered on the Federal Register of Legislation.

*Note* The Federal Register of Legislation may be accessed at https://www.legislation.gov.au.

3 Authority

 This Variation is made under subsection 132(1) of the *Radiocommunications Act 1992*.

4 Amendments

 The instrument that is specified in Schedule 1 is varied as set out in the applicable items in that Schedule.

Schedule 1—Variations

(section 4)

Radiocommunications (Citizen Band Radio Stations) Class Licence 2015 (F2015L00876)

[1] Subsection 4(1), definition of *CB repeater station*, paragraph (a)

omit

established

insert

operating

[2] Subsection 5(1)

substitute

Subject to sections 6, 7, 8, 9, 10 and 11 a person may operate a CB station of a kind to which subsection (2), (3), (4), (5) or (6) applies.

[3] Paragraph 6(i)

omit

[4] Schedule 1, Item 5

substitute

|  |  |  |  |
| --- | --- | --- | --- |
| 5 | 123456783132333435363738 | 476.4250476.4500476.4750476.5000476.5250476.5500476.5750476.6000477.1750477.2000477.2250477.2500477.2750477.3000477.3250477.3500 |  (a) Operation of a CB station must only employ F3E or G3E with a transmitter power not exceeding 5 watts pZ and with a necessary bandwidth not exceeding 16 kHz. (b) The use of audio tones, including subaudible tones, for initiating communications with another CB station, is not authorised on channel 35.*Note Channels 1-8 are for the automatic re-transmission of radio signals from CB stations. Channels 31-38 are for the reception of radio signals from CB stations.* |

[5] Schedule 1, Item 8

*substitute*

|  |  |  |  |
| --- | --- | --- | --- |
| 8 | 123456783132333435363738 | 476.4250476.4500476.4750476.5000476.5250476.5500476.5750476.6000477.1750477.2000477.2250477.2500477.2750477.3000477.3250477.3500 |  (a) Operation of a CB station must only employ F3E or G3E with a transmitter power not exceeding 5 watts pZ and with a necessary bandwidth not exceeding 10.1 kHz. (b) The use of audio tones, including subaudible tones, for initiating communications with another CB station, is not authorised on channel 35.*Note Channels 1-8 and 41-48 are for the automatic re-transmission of radio signals from CB stations. Channels 31-38 and 71-78 are for the reception of radio signals from CB stations.* |
|  | 41424344454647487172737475767778 | 476.4375476.4625476.4875476.5125476.5375476.5625476.5875476.6125477.1875477.2125477.2375477.2625477.2875477.3125477.3375477.3625 |  |