

Vehicle Standard (Australian Design Rule 57/00 –Special Requirements for L-Group Vehicles) 2006 Amendment 1

I, PAUL FLETCHER, Minister for Territories, Local Government and Major Projects, determine this vehicle standard under section 7 of the *Motor Vehicle Standards Act 1989*.

Dated 11 November 2015

[Signed]

Paul Fletcher

Minister for Territories, Local Government and Major Projects

**CONTENTS**

[1. Legislative provisions 3](#_Toc433369165)

[2. Amendment of vehicle standard 3](#_Toc433369166)

[SCHEDULE 1 3](#_Toc433369167)

Legislative provisions

* 1. Name of Legislative Instrument
     1. This instrument is the Vehicle Standard (Australian Design Rule 57/00 –Special Requirements for L-Group Vehicles) 2006 Amendment 1
  2. Commencement
     1. This instrument commences on the day after it is registered.

Amendment of vehicle standard

* 1. The changes specified in Schedule 1 amend Vehicle Standard (Australian Design Rule 57/00 –Special Requirements for L-Group Vehicles) 2006.

SCHEDULE 1

1. Clause 57.2.2.1 amend to read:

“Handlebars must not extend:

1. less than 250mm on each side of the centreline of the vehicle for all L Group vehicles;
2. more than 450mm on each side of the centreline of the vehicle for LA, LB and LE category vehicles; or
3. more than 550mm on each side of the centreline of the vehicle for all LC and LD category vehicles.”