

Vehicle Standard (Australian Design Rule 57/00 – Special Requirements for L-Group Vehicles) 2006 Amendment 2

I, PAUL FLETCHER, Minister for Urban Infrastructure, determine this vehicle standard under section 7 of the *Motor Vehicle Standards Act 1989*.

Dated 7/11/2016

[SIGNED]

Paul Fletcher

Minister for Urban Infrastructure

**CONTENTS**

[1. Legislative provisions 3](#_Toc445378185)

[2. Amendment of vehicle standard 3](#_Toc445378186)

[SCHEDULE 1 3](#_Toc445378187)

Legislative provisions

* 1. Name of Legislative Instrument
		1. This instrument is the Vehicle Standard (Australian Design Rule 57/00 – Special Requirements for L-Group Vehicles) 2006 Amendment 2.
	2. Commencement
		1. This instrument commences on the day after it is registered.

Amendment of vehicle standard

* 1. The changes specified in Schedule 1 amend Vehicle Standard (Australian Design Rule 57/00 – Special Requirements for L-Group Vehicles) 2006.

SCHEDULE 1

1. Clause C1.2. Applicability Table amend to read (footnote \* remains the same):

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Vehicle Category** | **ADR Category Code \*** | **UNECE Category Code \*** | **Manufactured on or After** | **Acceptable Prior Rules** |
| Moped 2 wheels | LA | L1 | 1 July 1988 | Nil |
| Moped 3 wheels | LB | L2 | Not applicable |  |
| Motor cycle | LC | L3 | 1 July 1988 | Nil |
| Motor cycle and sidecar | LD | L4 | 1 July 1988 | Nil |
| Motor tricycle | LE | L5 | Not applicable |  |
| Passenger car | MA | M1 | Not applicable |  |
| Forward-control passenger vehicle | MB | M1 | Not applicable |  |
| Off-road passenger vehicle | MC | M1 | Not applicable |  |
| Light omnibus | MD | M2 | Not applicable |  |
| Heavy omnibus | ME | M3 | Not applicable |  |
| Light goods vehicle | NA | N1 | Not applicable |  |
| Medium goods vehicle | NB | N2 | Not applicable |  |
| Heavy goods vehicle | NC | N3 | Not applicable |  |
| Very light trailer | TA | O1 | Not applicable |  |
| Light trailer | TB | O2 | Not applicable |  |
| Medium trailer | TC | O3 | Not applicable |  |
| Heavy trailer | TD | O4 | Not applicable |  |

1. Clause 57.2.2.1 amend to read:

“Handlebars must not extend:

1. less than 250mm on each side of the centreline of the vehicle for all LA, LC and LD category vehicles;
2. more than 450mm on each side of the centreline of the vehicle for LA category vehicles; or
3. more than 550mm on each side of the centreline of the vehicle for all LC and LD category vehicles.”