

Vehicle Standard (Australian Design Rule 45/01 – Lighting and Light Signalling Devices not Covered by ECE Regulations) 2006 Amendment 1

I, PAUL FLETCHER, Minister for Urban Infrastructure, determine this vehicle standard under section 7 of the *Motor Vehicle Standards Act 1989*.

Dated 08/11/2017

(SIGNED)

PAUL FLETCHER

Minister for Urban Infrastructure

**CONTENTS**

1. legislative provisions 3

2. amendment of vehicle standard 3

Schedule 1 5

1. legislative provisions
   1. Name of Legislative Instrument
      1. This instrument is the Vehicle Standard (Australian Design Rule 45/01 – Lighting and Light Signalling Devices not Covered by ECE Regulations) 2006 Amendment 1.
   2. Commencement
      1. This instrument commences on the day after it is registered.
2. amendment of vehicle standard
   1. The changes specified in Schedule 1 amend Vehicle Standard (Australian Design Rule 45/01 – Lighting and Light Signalling Devices not Covered by ECE Regulations) 2006.

Schedule 1

1. Clause 0. and subclauses renumber to 1. and subclauses.
2. Clause “PURPOSE AND SCOPE” replace with “2. FUNCTION”
3. Number clause 2. subclause as 2.1.
4. Insert “(ADR)” after “Australian Design Rule” in clause 2.1.
5. Number “Applicability and Implementation” as Clause 3.
6. Number Clause 3. subclauses as 3.1., 3.2. and 3.3.
7. Replace Clause 3.2 with:

“3. ‘*External Cabin Lamps*’ shall comply with the relevant requirements of this ADR.”

1. Replace Clause 3.3 with:

“3.3. The circumstances under which such lamps are mandatory, optional, alternative or prohibited are set out in ADR 13/...”

1. Delete clause beginning “Vehicles certified to any of the “Acceptable Prior Rules”…”
2. Delete Applicability Table
3. Renumber clause 45.1. as clause 4.
4. Renumber clause 45.1.1. as clause 4.1.
5. Renumber clause 45.2. as clause 5.
6. Renumber clause 45.2.1. as clause 5.1.
7. Replace clause 45.2.2. with:

“5.2. The colour of the light emitted shall be in accordance with the chromaticity requirements within Appendix A of Vehicle Standard (Australian Design Rule 13/00 – Installation of Lighting and Light Signalling Devices on other than L-Group Vehicles) 2005.”

1. Delete clauses 45.2.2.1. and 45.2.2.2.
2. Renumber clause 45.3. as clause 6.
3. Delete clause 45.3.1. and subclauses.
4. Renumber clause 45.3.2. as clause 6.1.
5. Renumber clause 45.3.2.1. as clause 6.1.1.
6. Replace clause 6.1.1. with:

“6.1.1. Colour of light emitted: White or Amber”

1. Renumber clause 45.3.2.2. as clause 6.1.2.
2. Renumber clause 45.3.2.2.1. as clause 6.1.2.1.
3. Renumber clause 45.3.2.2.2. as clause 6.1.2.2.
4. Renumber clause 45.3.2.3. as clause 6.1.3.
5. Renumber clause 45.3.2.3.1. as clause 6.1.3.1.
6. Renumber clause 45.3.2.3.2. as clause 6.1.3.2.
7. Renumber clause 45.3.2.4. as clause 6.1.4.
8. Delete clause 45.3.3. and subclauses.
9. Delete clause 45.3.4. and subclauses.
10. Delete clause 45.3.5. and subclauses.
11. Delete clause 45.3.6. and subclauses.
12. Delete clause 45.3.7. and subclauses.
13. Delete clause 45.3.8. and subclauses.
14. Delete clause 45.3.9. and subclauses.
15. Renumber clause 45.4. as clause 7.
16. Renumber clause 45.4.1. as clause 7.1.
17. Replace clause 7.1. with:

“7. All measurements shall be made with a standard filament globe of the category prescribed for the device, or LED light source as specified by the manufacturer, the supply voltage being so regulated as to produce the normal luminous flux prescribed. In the case that the LED light source is fitted to the unit and not removable, the unit shall be tested as supplied at the voltage specified by the manufacturer.”

1. Renumber clause 45.4.2. as clause 7.2.
2. Renumber clause 45.4.2.1. as clause 7.2.1.
3. Renumber clause 45.4.2.1.1. as clause 7.2.1.1.
4. Renumber clause 45.4.2.1.2. as clause 7.2.1.2.
5. Renumber clause 45.4.2.1.2.1. as clause 7.2.1.2.1.
6. Renumber clause 45.4.2.1.2.2. as clause 7.2.1.2.2.
7. Renumber clause 45.4.2.1.2.3. as clause 7.2.1.2.3.